|  | General |
Study name
mold_20design2_5fc19_5finv_5ftut01_5fmp_2eipt_gate.sdy
Study location
C:\Inventor_2017\c19\AIT\Mold\Moldflow\Mold_20Design2_2Eiam\mold_20design2_5fc19_5finv_5ftut01_5fmp_2eipt_gate.sdy
Part name
Mold_20Design2_5Fc19_5FInv_5Ftut01_5FMP_2Eipt_gate
Model suitability
The imported model is thin walled, and is appropriate for Dual-Domain analysis.
Analysis resolution
Default
Material

Material manufacturer
A Schulman Plastics (Dongguan) Ltd
Material trade name
Schulamid 6 GF15 SHI K1946 JETBLACK 96.7762
Environmental impact

Melt temperature
258.0 (C)
Mold temperature
75.0 (C)
Injection locations
0
Max. machine injection pressure
180.000 (MPa)

Model warnings
None