|  | General |
Study name
mold_20design1_5fc19_5finv_5ftut01_5fmp_2eipt_mwindow.sdy
Study location
C:\Inventor_2017\c19\AIT\Mold\Moldflow\Mold_20Design1_2Eiam\mold_20design1_5fc19_5finv_5ftut01_5fmp_2eipt_mwindow.sdy
Part name
Mold_20Design1_5Fc19_5FInv_5Ftut01_5FMP_2Eipt_mwindow
Model suitability
The imported model is thin walled, and is appropriate for Dual-Domain analysis.
Analysis resolution
Default
Material

Material manufacturer
SABIC Innovative Plastics US, LLC
Material trade name
Cycolac G360
Environmental impact

Melt temperature
240.0 (C)
Mold temperature
65.0 (C)
Injection locations
3
Max. machine injection pressure
180.000 (MPa)

Model warnings
None