

 Autodesk (R) Simulation Static Stress with Linear Material Models
 Version 2015.00.00.0517-W64/X64 26-Feb-2014
 Copyright (c) 2014, Autodesk, Inc. All rights reserved. 

 
                          DATE: JULY 21, 2014                 
                          TIME: 05:47 PM
                   INPUT MODEL: D:\Autodesk Simulation Manuscript\Autodesk Simulation Manuscript 2015\Autodesk Simulation _Tut and Exe_Final - Used\Input File\c06_simulation_2014_input\Tut03\c06_tut03.ds_data\1\ds

                    PROGRAM VERSION: 201500000517
            alg-win-x64.dll VERSION: 201500000516
       agsdb_ar-win-x64.dll VERSION: 201500000516
      algconfig-win-x64.dll VERSION: 201500000516
 solvercallback-win-x64.dll VERSION: 201500000516
               amgsolve.exe VERSION:    360000000
 
 **** Linear stress analysis
 **** Nodes    | Parts | Loads | Freqs | Mode
           3707|      1|      1|      0|    0

 **** Model Unit System Settings:
      --------------------------------------------
       Unit System              : Custom
       Force                    : N
       Length                   : mm
       Time                     : s
       Temperature (Absolute)   : deg C (K)
       Thermal Energy           : J
       Voltage                  : V
       Current                  : A
       Electrical Resistance    : ohm
       Mass                     : N*s^2/mm
      --------------------------------------------

  
      Options executed are: 
  
      NOMIN
      STRAIN
      SPARSE
      SUPCNF
      SUPELM
      SUPNOD
      REAC
  
  
      processing ... 
  
 **** OPENING TEMPORARY FILES
      NDYN = 0 
 **** BEGIN NODAL DATA INPUT
      3707 NODES
      10701 DOFS               
 **** END   NODAL DATA INPUT
 
 **** Begin brick element (TYPE-8) data input
 **** Part      1 containing      7292 elements
             0 ( 0.%) elements
                                                 
 **** End input of element part      1

 **** Hard disk file size information for processor:

      Available hard disk space on current drive = 121811.891 megabytes


 
 **** BEGIN LOAD INPUT
      Gravity direction vector =  0.0000E+00  0.0000E+00 -1.0000E+00
      One load case.
 **** END   LOAD INPUT

 **** Symbolic Assembly Using the Row-Hits Matrix Profile ...
 **** Number of equations                 = 10701
      Estimated maximum bandwidth         = 1311
      Estimated triangle matrix nonzeroes = 1828854
      Symbolically assembled nonzeros     = 265338
 **** Real Sparse Matrix Assembly ...
      in the upper triangle:
      number of entries in the profile    = 1828854
      number of nonzeros                  = 265300

 **** Sparse Matrix Assembled

 **** Invoking Parallel BCSLIB-EXT Sparse Solver...
 
 **** Load Cases 1
 **** End Sparse Solver Solution
 
 **** BEGIN DISPLACEMENT OUTPUT
 **** PRINT OF DISPLACEMENT OUTPUT SUPPRESSED
 **** END   DISPLACEMENT OUTPUT
 
 **** BEGINNING REACTION COMPUTATIONS
 **** LOADCASES REMAINING      1 
 **** PARTS REMAINING       1 
 **** ELEMENT/GLOBAL CONTRIBUTIONS Part = 1 
      THE 1st PART CONTAINING 7292 ELEMENTS
                                                 
 **** ENDING REACTION COMPUTATIONS

      Processing completed ... 

 
      ds.t7    =      83.602 kilobytes
      ds.t8    =     173.871 kilobytes
      ds.t9    =       0.000 kilobytes
      ds.t10   =       0.000 kilobytes
      ds.t11   =       0.000 kilobytes
      ds.t12   =      83.602 kilobytes
      ds.t13   =      83.609 kilobytes
      ds.t14   =       0.000 kilobytes
      ds.t15   =       0.000 kilobytes
      ds.t17   =       0.000 kilobytes
      ds.t50   =   10994.969 kilobytes
      ds.t51   =     911.500 kilobytes
      ds.t52   =   17147.594 kilobytes
      ds.t54   =      41.824 kilobytes
      ds.t55   =    1036.328 kilobytes
      ds.t56   =    2072.656 kilobytes
      ds.t56   =    2072.656 kilobytes
      ds.t58   =       0.000 kilobytes
      ds.t59   =       0.000 kilobytes
 
      total temporary disk storage (megabytes) = 33.889 
 
      ds.l     =       7.571 kilobytes
      ds.do    =     173.812 kilobytes
 
 **** BEGIN DELETING TEMPORARY FILES
 **** TEMPORARY FILES DELETED
 **** END OF SUCCESSFUL EXECUTION
 
 

 **** Total actual hard disk space used    =     34.066 megabytes

      Sub-total elapsed time               =      0.040 minutes



 Autodesk (R) Simulation Stress Calculation Utility
 Version 2015.00.00.0517-W64/X64 26-Feb-2014
 Copyright (c) 2014, Autodesk, Inc. All rights reserved. 


      DATE: JULY 21, 2014                 
      TIME: 05:48 PM
      INPUT......D:\Autodesk Simulation Manuscript\Autodesk Simulation Manuscript 2015\Autodesk Simulation _Tut and Exe_Final - Used\Input File\c06_simulation_2014_input\Tut03\c06_tut03.ds_data\1\ds 

 **** Model Unit System Settings:
      --------------------------------------------
       Unit System              : Custom
       Force                    : N
       Length                   : mm
       Time                     : s
       Temperature (Absolute)   : deg C (K)
       Thermal Energy           : J
       Voltage                  : V
       Current                  : A
       Electrical Resistance    : ohm
       Mass                     : N*s^2/mm
      --------------------------------------------


 **** START PROCESSING ELEMENTS 

 **** BEGIN PART   1 TYPE( 8) ELEMENTS
      7292 ELEMENTS
          4220 (58.%) elements
          3196 (44.%) elements
          1148 (16.%) elements
                                                 

 **** FINISHED PROCESSING ELEMENTS 

 **** Hard disk file size information for postprocessor:
      ds.nso   =    2050.945 kilobytes
      ds.sto   =    2050.945 kilobytes

      Total MKNSO disk space used        =     4.00575 megabytes
 **** MKNSO elapsed time                 =       0.044 minutes

 **** The TOTAL elapsed time             =       0.084 minutes

 
