TSX2TSY Version 2015.0 20-Feb-2014
Copyright (c) 2014, Autodesk, Inc. All rights reserved.

    Time:	07/14/14 18:25:34

    Input : D:\Autodesk Simulation Manuscript\Autodesk Simulation Manuscript 2015\Autodesk Simulation _Tut and Exe_Final - Used\Input File\c07_simulation_2014_input\Tut02\c07_tut02.fem
    Output: D:\Autodesk Simulation Manuscript\Autodesk Simulation Manuscript 2015\Autodesk Simulation _Tut and Exe_Final - Used\Input File\c07_simulation_2014_input\Tut02\c07_tut02.fem

    Command Line: "-a=100" -t=-0.316188 D:\Autodesk Simulation Manuscript\Autodesk Simulation Manuscript 2015\Autodesk Simulation _Tut and Exe_Final - Used\Input File\c07_simulation_2014_input\Tut02\c07_tut02.tsx -ds=1
    Shortest/Longest line in Part 1 : 2.221579 / 11.472289
    Shortest/Longest line in Part 2 : 4.153152 / 15.000000
    Shortest/Longest line in Part 3 : 0.720948 / 24.591399
    Shortest/Longest line in Part 4 : 1.892213 / 11.516731
    Shortest/Longest line in Part 5 : 1.892213 / 11.516731
    Shortest/Longest line in Part 6 : 1.525150 / 12.742017
    Shortest/Longest line in Part 7 : 1.525150 / 12.885464
    Node matching tolerance: 0.316188
    Found 371 matched corner node pairs.

    Duration: 1 seconds

