
Meshing Curves ...
 516 curves, 198 faces, Mesh size = 6.32376 (30.77 %)  
 Turnaround time:    0.000 seconds; Execution time:    0.441 seconds 
    DIMENSION_BASED_MESHING_CURVE

Meshing part 4 ...
 409 elements, 21 surfaces, 28 faces, Mesh size = 8.09228 (124.82 %)  
 Turnaround time:    1.360 seconds; Execution time:    0.174 seconds 
    DIMENSION_BASED_MESHING_SURFACE

Meshing part 5 ...
 412 elements, 21 surfaces, 28 faces, Mesh size = 8.09228 (124.82 %)  
 Turnaround time:    0.137 seconds; Execution time:    0.140 seconds 
    DIMENSION_BASED_MESHING_SURFACE

Meshing part 6 ...
      Meshed part 6 face 3 (surface 8) by copying mesh from part 5 face 17 (surface 11)
      Meshed part 6 face 4 (surface 10) by copying mesh from part 5 face 19 (surface 12)
 646 elements, 30 surfaces, 38 faces, Mesh size = 9.05991 (121.09 %)  
 Turnaround time:    0.138 seconds; Execution time:    0.661 seconds 
    DIMENSION_BASED_MESHING_SURFACE

Meshing part 7 ...
      Meshed part 7 face 3 (surface 10) by copying mesh from part 4 face 17 (surface 11)
      Meshed part 7 face 4 (surface 8) by copying mesh from part 4 face 19 (surface 12)
 641 elements, 30 surfaces, 38 faces, Mesh size = 9.05991 (121.09 %)  
 Turnaround time:    0.150 seconds; Execution time:    0.242 seconds 
    DIMENSION_BASED_MESHING_SURFACE

Meshing part 1 ...
      Meshed part 1 face 16 (surface 9) by copying mesh from part 5 face 1 (surface 6)
      Meshed part 1 face 18 (surface 10) by copying mesh from part 5 face 2 (surface 8)
      Meshed part 1 face 25 (surface 16) by copying mesh from part 4 face 1 (surface 8)
      Meshed part 1 face 27 (surface 17) by copying mesh from part 4 face 2 (surface 6)
 1211 elements, 17 surfaces, 27 faces, Mesh size = 8 (133.33 %)  
 Turnaround time:    0.192 seconds; Execution time:    0.208 seconds 
    DIMENSION_BASED_MESHING_SURFACE

Meshing part 2 ...
      Meshed part 2 face 1 (surface 2) by copying mesh from part 1 face 6 (surface 4)
      Meshed part 2 face 2 (surface 2) by copying mesh from part 1 face 7 (surface 4)
      Meshed part 2 face 3 (surface 2) by copying mesh from part 1 face 8 (surface 4)
      Meshed part 2 face 4 (surface 2) by copying mesh from part 1 face 9 (surface 4)
      Meshed part 2 face 5 (surface 3) by copying mesh from part 1 face 14 (surface 8)
 699 elements, 5 surfaces, 17 faces, Mesh size = 10.8889 (192.89 %)  
 Turnaround time:    0.125 seconds; Execution time:    0.149 seconds 
    DIMENSION_BASED_MESHING_SURFACE

Meshing part 3 ...
      Meshed part 3 face 1 (surface 4) by copying mesh from part 2 face 12 (surface 2)
      Meshed part 3 face 2 (surface 4) by copying mesh from part 2 face 13 (surface 2)
      Meshed part 3 face 3 (surface 4) by copying mesh from part 2 face 14 (surface 2)
      Meshed part 3 face 4 (surface 4) by copying mesh from part 2 face 15 (surface 2)
      Meshed part 3 face 20 (surface 11) by copying mesh from part 7 face 1 (surface 14)
      Meshed part 3 face 22 (surface 12) by copying mesh from part 7 face 2 (surface 16)
      Meshed part 3 face 28 (surface 17) by copying mesh from part 6 face 1 (surface 14)
      Meshed part 3 face 30 (surface 18) by copying mesh from part 6 face 2 (surface 16)
 1817 elements, 31 surfaces, 43 faces, Mesh size = 15.3413 (188.45 %)  
 Turnaround time:    0.173 seconds; Execution time:    0.342 seconds 
    DIMENSION_BASED_MESHING_SURFACE

Total time: 5 seconds. 07/14/14 18:25:34. TSMESH V2015.0, 20-Feb-2014.
=========================================================================

