TSX2TSY Version 2015.0 20-Feb-2014
Copyright (c) 2014, Autodesk, Inc. All rights reserved.

    Time:	07/14/14 18:19:44

    Input : D:\Autodesk Simulation Manuscript\Autodesk Simulation Manuscript 2015\Autodesk Simulation _Tut and Exe_Final - Used\Input File\c07_simulation_2014_input\Tut01\c07_tut01.fem
    Output: D:\Autodesk Simulation Manuscript\Autodesk Simulation Manuscript 2015\Autodesk Simulation _Tut and Exe_Final - Used\Input File\c07_simulation_2014_input\Tut01\c07_tut01.fem

    Command Line: "-a=100" -t=-0.100426 D:\Autodesk Simulation Manuscript\Autodesk Simulation Manuscript 2015\Autodesk Simulation _Tut and Exe_Final - Used\Input File\c07_simulation_2014_input\Tut01\c07_tut01.tsx -ds=1
    Shortest/Longest line in Part 1 : 0.006019 / 6.899783
    Shortest/Longest line in Part 2 : 0.281611 / 4.890781
    Node matching tolerance: 0.100426
    Found 0 matched corner node pairs.

    Duration: 0 seconds

