
Meshing Curves ...
 516 curves, 198 faces, Mesh size = 6 (29.19 %)  
 Turnaround time:    0.000 seconds; Execution time:    0.227 seconds 
    DIMENSION_BASED_MESHING_CURVE

Meshing part 4 ...
 750 elements, 21 surfaces, 28 faces, Mesh size = 6 (92.55 %)  
 Turnaround time:    0.706 seconds; Execution time:    0.101 seconds 
    DIMENSION_BASED_MESHING_SURFACE

Meshing part 5 ...
 750 elements, 21 surfaces, 28 faces, Mesh size = 6 (92.55 %)  
 Turnaround time:    0.129 seconds; Execution time:    0.155 seconds 
    DIMENSION_BASED_MESHING_SURFACE

Meshing part 6 ...
      Meshed part 6 face 3 (surface 8) by copying mesh from part 5 face 17 (surface 11)
      Meshed part 6 face 4 (surface 10) by copying mesh from part 5 face 19 (surface 12)
 1104 elements, 30 surfaces, 38 faces, Mesh size = 6 (80.19 %)  
 Turnaround time:    0.151 seconds; Execution time:    0.175 seconds 
    DIMENSION_BASED_MESHING_SURFACE

Meshing part 7 ...
      Meshed part 7 face 3 (surface 10) by copying mesh from part 4 face 17 (surface 11)
      Meshed part 7 face 4 (surface 8) by copying mesh from part 4 face 19 (surface 12)
 1107 elements, 30 surfaces, 38 faces, Mesh size = 6 (80.19 %)  
 Turnaround time:    0.087 seconds; Execution time:    0.155 seconds 
    DIMENSION_BASED_MESHING_SURFACE

Meshing part 1 ...
      Meshed part 1 face 16 (surface 9) by copying mesh from part 5 face 1 (surface 6)
      Meshed part 1 face 18 (surface 10) by copying mesh from part 5 face 2 (surface 8)
      Meshed part 1 face 25 (surface 16) by copying mesh from part 4 face 1 (surface 8)
      Meshed part 1 face 27 (surface 17) by copying mesh from part 4 face 2 (surface 6)
 1917 elements, 17 surfaces, 27 faces, Mesh size = 6 (100.00 %)  
 Turnaround time:    0.088 seconds; Execution time:    0.218 seconds 
    DIMENSION_BASED_MESHING_SURFACE

Meshing part 2 ...
      Meshed part 2 face 1 (surface 2) by copying mesh from part 1 face 6 (surface 4)
      Meshed part 2 face 2 (surface 2) by copying mesh from part 1 face 7 (surface 4)
      Meshed part 2 face 3 (surface 2) by copying mesh from part 1 face 8 (surface 4)
      Meshed part 2 face 4 (surface 2) by copying mesh from part 1 face 9 (surface 4)
      Meshed part 2 face 5 (surface 3) by copying mesh from part 1 face 14 (surface 8)
 1879 elements, 5 surfaces, 17 faces, Mesh size = 6 (106.29 %)  
 Turnaround time:    0.071 seconds; Execution time:    0.184 seconds 
    DIMENSION_BASED_MESHING_SURFACE

Meshing part 3 ...
      Meshed part 3 face 1 (surface 4) by copying mesh from part 2 face 12 (surface 2)
      Meshed part 3 face 2 (surface 4) by copying mesh from part 2 face 13 (surface 2)
      Meshed part 3 face 3 (surface 4) by copying mesh from part 2 face 14 (surface 2)
      Meshed part 3 face 4 (surface 4) by copying mesh from part 2 face 15 (surface 2)
      Meshed part 3 face 20 (surface 11) by copying mesh from part 7 face 1 (surface 14)
      Meshed part 3 face 22 (surface 12) by copying mesh from part 7 face 2 (surface 16)
      Meshed part 3 face 28 (surface 17) by copying mesh from part 6 face 1 (surface 14)
      Meshed part 3 face 30 (surface 18) by copying mesh from part 6 face 2 (surface 16)
 8471 elements, 31 surfaces, 43 faces, Mesh size = 6 (73.70 %)  
 Turnaround time:    0.093 seconds; Execution time:    1.110 seconds 
    DIMENSION_BASED_MESHING_SURFACE

Total time: 3 seconds. 03/19/13 16:33:14. TSMESH V2014.0, 08-Nov-2012.
=========================================================================


Meshing Curves ...
 516 curves, 198 faces, Mesh size = 6 (29.19 %)  
 Turnaround time:    0.000 seconds; Execution time:    0.233 seconds 
    DIMENSION_BASED_MESHING_CURVE

Meshing part 4 ...
 750 elements, 21 surfaces, 28 faces, Mesh size = 6 (92.55 %)  
 Turnaround time:    1.036 seconds; Execution time:    0.100 seconds 
    DIMENSION_BASED_MESHING_SURFACE

Meshing part 5 ...
 750 elements, 21 surfaces, 28 faces, Mesh size = 6 (92.55 %)  
 Turnaround time:    0.096 seconds; Execution time:    0.099 seconds 
    DIMENSION_BASED_MESHING_SURFACE

Meshing part 6 ...
      Meshed part 6 face 3 (surface 8) by copying mesh from part 5 face 17 (surface 11)
      Meshed part 6 face 4 (surface 10) by copying mesh from part 5 face 19 (surface 12)
 1104 elements, 30 surfaces, 38 faces, Mesh size = 6 (80.19 %)  
 Turnaround time:    0.067 seconds; Execution time:    0.152 seconds 
    DIMENSION_BASED_MESHING_SURFACE

Meshing part 7 ...
      Meshed part 7 face 3 (surface 10) by copying mesh from part 4 face 17 (surface 11)
      Meshed part 7 face 4 (surface 8) by copying mesh from part 4 face 19 (surface 12)
 1107 elements, 30 surfaces, 38 faces, Mesh size = 6 (80.19 %)  
 Turnaround time:    0.065 seconds; Execution time:    0.148 seconds 
    DIMENSION_BASED_MESHING_SURFACE

Meshing part 1 ...
      Meshed part 1 face 16 (surface 9) by copying mesh from part 5 face 1 (surface 6)
      Meshed part 1 face 18 (surface 10) by copying mesh from part 5 face 2 (surface 8)
      Meshed part 1 face 25 (surface 16) by copying mesh from part 4 face 1 (surface 8)
      Meshed part 1 face 27 (surface 17) by copying mesh from part 4 face 2 (surface 6)
 1917 elements, 17 surfaces, 27 faces, Mesh size = 6 (100.00 %)  
 Turnaround time:    0.301 seconds; Execution time:    0.218 seconds 
    DIMENSION_BASED_MESHING_SURFACE

Meshing part 2 ...
      Meshed part 2 face 1 (surface 2) by copying mesh from part 1 face 6 (surface 4)
      Meshed part 2 face 2 (surface 2) by copying mesh from part 1 face 7 (surface 4)
      Meshed part 2 face 3 (surface 2) by copying mesh from part 1 face 8 (surface 4)
      Meshed part 2 face 4 (surface 2) by copying mesh from part 1 face 9 (surface 4)
      Meshed part 2 face 5 (surface 3) by copying mesh from part 1 face 14 (surface 8)
 1879 elements, 5 surfaces, 17 faces, Mesh size = 6 (106.29 %)  
 Turnaround time:    0.080 seconds; Execution time:    0.186 seconds 
    DIMENSION_BASED_MESHING_SURFACE

Meshing part 3 ...
      Meshed part 3 face 1 (surface 4) by copying mesh from part 2 face 12 (surface 2)
      Meshed part 3 face 2 (surface 4) by copying mesh from part 2 face 13 (surface 2)
      Meshed part 3 face 3 (surface 4) by copying mesh from part 2 face 14 (surface 2)
      Meshed part 3 face 4 (surface 4) by copying mesh from part 2 face 15 (surface 2)
      Meshed part 3 face 20 (surface 11) by copying mesh from part 7 face 1 (surface 14)
      Meshed part 3 face 22 (surface 12) by copying mesh from part 7 face 2 (surface 16)
      Meshed part 3 face 28 (surface 17) by copying mesh from part 6 face 1 (surface 14)
      Meshed part 3 face 30 (surface 18) by copying mesh from part 6 face 2 (surface 16)
 8471 elements, 31 surfaces, 43 faces, Mesh size = 6 (73.70 %)  
 Turnaround time:    0.099 seconds; Execution time:    1.110 seconds 
    DIMENSION_BASED_MESHING_SURFACE

Total time: 5 seconds. 03/19/13 17:19:34. TSMESH V2014.0, 08-Nov-2012.
=========================================================================

