fem2esh - Make esh file from fem file for a specified design scenario
Version 2014.00.00.0513-W64/X64 22-Feb-2013
Copyright (c) 2013, Autodesk, Inc. All rights reserved.

  Version of fem2esh.exe          : 2014.00000513
  Version of dcx1-win-x64.dll     : 2014.00000513
  Version of femapi-win-x64.dll   : 2014.00000513
  Version of agsdb_ar-win-x64.dll : 2014.00000513
  Version of tsx2tsy.exe          : 2014.00000513

  Input Model     : D:\Autodesk Simulation Manuscript\c08_Autodesk-Simulation\tut02\c08_tut02.ds_data\1\ds
  Input File      : D:\Autodesk Simulation Manuscript\c08_Autodesk-Simulation\tut02\c08_tut02.fem
  Output File     : D:\Autodesk Simulation Manuscript\c08_Autodesk-Simulation\tut02\c08_tut02.ds_data\1\ds.mod\group.esh
  Log File        : D:\Autodesk Simulation Manuscript\c08_Autodesk-Simulation\tut02\c08_tut02.ds_data\1\ds.mod\group.ldx
  Design scenario : 1
  Analysis type   : Linear Stress
  Start time      : 2013/09/23-14:38:46  

  --- Get 3 active element parts in range [1, 3] from fem file
  --- 3 enabled L&C groups are defined
  --- Get 23588 points defined in range [1, 23667] from fem file
  Calling the Surface Topology Generator (tsx2tsy)...
  tsx2tsy: Update part surface contact/bonding data (duration=0 sec.)
  --- No mid-side node required
  Set up nodal properties such as admissible BC etc. by adjacent elements...
  --- Load up 228 non-trivial coincident nodal pairs of 228 in FEM
  Consolidate points between parts using contact definitions...
  --- No contact used from 0 contact definitions
  Compress FEM points to ESH nodes...
  --- Found 12669 independent nodes
  --- 12669 mesh nodes formed from 23588 FEM points
  Output the mapping arrays of FEM points to FEA nodes...
  Add user defined nodal B.C.'s...
  --- Found 331 out of 502 defined nodal BC's are not in use, ignored
  --- No contact found
  Get beam loads and constraints data...
  Writing to ESH file in phase I (nodes & elements)...
  --- Part1: type=8, flags=7, meshType=10, elements=10409, maximumID=10409
  --- Part2: type=8, flags=7, meshType=10, elements=9463, maximumID=9463
  --- Part3: type=1, flags=7, meshType=11, elements=456, maximumID=912
  Working on MPCs...
  --- No MPC made in the model.
  Writing to ESH file in phase II (FEA objects)...
  Found defined elastic BE are not in use, ignored 64 out of 232
  Use global coordinate system, no local coordinate system defined.


  == Model Stats ==

  FEA Nodes & Elements:
  --- 12669 mesh nodes
      + 84 extral nodes
  --- 228 nodes bonded.
  --- 3 parts and total 20328 elements
  FEA Object (total made 339):
  --- User Defined Boundary Conditions: 171
  --- Elastic Boundary Elements: 168
  FEM2ESH Duration: 1 seconds (CPU time)

2013/09/23-14:38:47