

 Autodesk (R) Simulation Static Stress with Linear Material Models
 Version 2014.00.00.0513-W64/X64 22-Feb-2013
 Copyright (c) 2013, Autodesk, Inc. All rights reserved. 

 
                          DATE: SEPTEMBER 23, 2013            
                          TIME: 02:38 PM
                   INPUT MODEL: D:\Autodesk Simulation Manuscript\c08_Autodesk-Simulation\tut02\c08_tut02.ds_data\1\ds

                    PROGRAM VERSION: 201400000513
            alg-win-x64.dll VERSION: 201400000513
       agsdb_ar-win-x64.dll VERSION: 201400000513
      algconfig-win-x64.dll VERSION: 201400000513
 solvercallback-win-x64.dll VERSION: 201400000513
               amgsolve.exe VERSION:    360000000
 
 **** Linear stress analysis
 **** Nodes    | Parts | Loads | Freqs | Mode
          12753|      4|      1|      0|    0

 **** Model Unit System Settings:
      --------------------------------------------
       Unit System              : Custom
       Force                    : N
       Length                   : mm
       Time                     : s
       Temperature (Absolute)   : deg C (K)
       Thermal Energy           : J
       Voltage                  : V
       Current                  : A
       Electrical Resistance    : ohm
       Mass                     : N*s^2/mm
      --------------------------------------------

  
      Options executed are: 
  
      NOMIN
      STRAIN
      SPARSE
      SUPCNF
      SUPELM
      SUPNOD
      REAC
  
  
      processing ... 
  
 **** OPENING TEMPORARY FILES
      NDYN = 0 
 **** BEGIN NODAL DATA INPUT
      12753 NODES
      37494 DOFS               
 **** END   NODAL DATA INPUT
 
 **** Begin brick element (TYPE-8) data input
 **** Part      1 containing     10409 elements
                                                 
 **** End input of element part      1

 **** Begin brick element (TYPE-8) data input
 **** Part      2 containing      9463 elements
                                                 
 **** End input of element part      2

 **** Begin truss element (TYPE-1) data input
 **** Part      3 containing       456 elements
                                                 
 **** End input of element part      3

 **** Begin boundary element TYPE-7 data input
 **** Part      4 containing        84 elements
 **** End input of element part      4

 **** Hard disk file size information for processor:

      Available hard disk space on current drive = 149589.500 megabytes


 
 **** BEGIN LOAD INPUT
      Gravity direction vector =  0.0000E+00  0.0000E+00 -1.0000E+00
      One load case in 2 blocks.
 **** END   LOAD INPUT

 **** Symbolic Assembly Using the Row-Hits Matrix Profile ...
 **** Number of equations                 = 37494
      Estimated maximum bandwidth         = 1392
      Estimated triangle matrix nonzeroes = 5250228
      Symbolically assembled nonzeros     = 1182402
 **** Real Sparse Matrix Assembly ...
      in the upper triangle:
      number of entries in the profile    = 5250228
      number of nonzeros                  = 1182018

 **** Sparse Matrix Assembled

 **** Invoking Parallel BCSLIB-EXT Sparse Solver...
 
 **** Load Cases 1
 **** End Sparse Solver Solution
 
 **** BEGIN DISPLACEMENT OUTPUT
 **** PRINT OF DISPLACEMENT OUTPUT SUPPRESSED
 **** END   DISPLACEMENT OUTPUT
 
 **** BEGINNING REACTION COMPUTATIONS
 **** LOADCASES REMAINING      1 
 **** PARTS REMAINING       4 
 **** ELEMENT/GLOBAL CONTRIBUTIONS Part = 1 
      THE 1st PART CONTAINING 10409 ELEMENTS
             0 ( 0.%) elements
                                                 
 **** PARTS REMAINING       3 
 **** ELEMENT/GLOBAL CONTRIBUTIONS Part = 2 
      THE 2nd PART CONTAINING 9463 ELEMENTS
                                                 
 **** PARTS REMAINING       2 
 **** ELEMENT/GLOBAL CONTRIBUTIONS Part = 3 
      THE 3rd PART CONTAINING 456 ELEMENTS
                                                 
 **** PARTS REMAINING       1 
 **** PART IGNORED! NPAR(12) = -1  Part = 4 
      THE 4th PART CONTAINING 84 ELEMENTS
                                                 
 **** ENDING REACTION COMPUTATIONS

      Processing completed ... 

 
      ds.t7    =     508.641 kilobytes
      ds.t8    =     597.902 kilobytes
      ds.t9    =       0.000 kilobytes
      ds.t10   =       0.000 kilobytes
      ds.t11   =       0.000 kilobytes
      ds.t12   =     292.922 kilobytes
      ds.t13   =     508.656 kilobytes
      ds.t14   =       0.000 kilobytes
      ds.t15   =       0.000 kilobytes
      ds.t17   =       0.000 kilobytes
      ds.t50   =   30094.031 kilobytes
      ds.t51   =    2513.531 kilobytes
      ds.t52   =   46823.062 kilobytes
      ds.t54   =     146.484 kilobytes
      ds.t55   =    4617.258 kilobytes
      ds.t56   =    9234.516 kilobytes
      ds.t56   =    9234.516 kilobytes
      ds.t58   =       0.000 kilobytes
      ds.t59   =       0.000 kilobytes
 
      total temporary disk storage (megabytes) = 102.121 
 
      ds.l     =       7.847 kilobytes
      ds.do    =     597.844 kilobytes
 
 **** BEGIN DELETING TEMPORARY FILES
 **** TEMPORARY FILES DELETED
 **** END OF SUCCESSFUL EXECUTION
 
 

 **** Total actual hard disk space used    =    102.712 megabytes

      Sub-total elapsed time               =      0.104 minutes



 Autodesk (R) Simulation Stress Calculation Utility
 Version 2014.00.00.0513-W64/X64 22-Feb-2013
 Copyright (c) 2013, Autodesk, Inc. All rights reserved. 


      DATE: SEPTEMBER 23, 2013            
      TIME: 02:39 PM
      INPUT......D:\Autodesk Simulation Manuscript\c08_Autodesk-Simulation\tut02\c08_tut02.ds_data\1\ds 

 **** Model Unit System Settings:
      --------------------------------------------
       Unit System              : Custom
       Force                    : N
       Length                   : mm
       Time                     : s
       Temperature (Absolute)   : deg C (K)
       Thermal Energy           : J
       Voltage                  : V
       Current                  : A
       Electrical Resistance    : ohm
       Mass                     : N*s^2/mm
      --------------------------------------------


 **** START PROCESSING ELEMENTS 

 **** BEGIN PART   1 TYPE( 8) ELEMENTS
      10409 ELEMENTS
             0 ( 0.%) elements
                                                 
 **** BEGIN PART   2 TYPE( 8) ELEMENTS
      9463 ELEMENTS
                                                 
 **** BEGIN PART   3 TYPE( 1) ELEMENTS
      456 ELEMENTS
                                                 
 **** BEGIN PART   4 TYPE( 7) ELEMENTS
      84 ELEMENTS
                                                 

 **** FINISHED PROCESSING ELEMENTS 

 **** Hard disk file size information for postprocessor:
      ds.nso   =    5593.371 kilobytes
      ds.sto   =    5593.371 kilobytes

      Total MKNSO disk space used        =    10.92455 megabytes
 **** MKNSO elapsed time                 =       0.029 minutes

 **** The TOTAL elapsed time             =       0.133 minutes

 
