

 Autodesk (R) Simulation Static Stress with Linear Material Models
 Version 2014.00.00.0206-W64/X64 08-Nov-2012
 Copyright (c) 2012, Autodesk, Inc. All rights reserved. 

 
                          DATE: MARCH 28, 2013                
                          TIME: 11:18 AM
                   INPUT MODEL: D:\Autodesk Simulation Manuscript-13032013\c08_Autodesk-Simulation\tut01\c08_tut01.ds_data\1\ds

                    PROGRAM VERSION: 201400000206
            alg-win-x64.dll VERSION: 201400000206
       agsdb_ar-win-x64.dll VERSION: 201400000206
      algconfig-win-x64.dll VERSION: 201400000206
 solvercallback-win-x64.dll VERSION: 201400000206
               amgsolve.exe VERSION:    360000000
 
 **** Linear stress analysis
 **** Nodes    | Parts | Loads | Freqs | Mode
          17652|      1|      1|      0|    0

 **** Model Unit System Settings:
      --------------------------------------------
       Unit System              : Custom
       Force                    : N
       Length                   : mm
       Time                     : s
       Temperature (Absolute)   : deg C (K)
       Thermal Energy           : J
       Voltage                  : V
       Current                  : A
       Electrical Resistance    : ohm
       Mass                     : N*s^2/mm
      --------------------------------------------

  
      Options executed are: 
  
      CHECK
      NOMIN
      STRAIN
      SPARSE
      SUPCNF
      SUPELM
      SUPNOD
      REAC
  
  
      processing ... 
  
 **** OPENING TEMPORARY FILES
      NDYN = 0 
 **** BEGIN NODAL DATA INPUT
      17652 NODES
      52676 DOFS               
 **** END   NODAL DATA INPUT
 
 **** Read      72 MPC's from CST file
 **** Penalty based MPC method is used
 **** Begin brick element (TYPE-8) data input
 **** Part      1 containing     50827 elements
         30000 (59.%) elements
         20000 (39.%) elements
         10000 (20.%) elements
             0 ( 0.%) elements
                                                 
 **** End input of element part      1

 **** Hard disk file size information for processor:

      Available hard disk space on current drive = 401570.938 megabytes


 
 **** BEGIN LOAD INPUT
      Gravity direction vector =  0.0000E+00  0.0000E+00 -1.0000E+00
      One load case in 3 blocks.
 **** END   LOAD INPUT

 **** Symbolic Assembly Using the Row-Hits Matrix Profile ...
 **** Number of equations                 = 52676
      Estimated maximum bandwidth         = 2833
      Estimated triangle matrix nonzeroes = 12994427
      Symbolically assembled nonzeros     = 1238248
 **** Real Sparse Matrix Assembly ...
      in the upper triangle:
      number of entries in the profile    = 12994643
      number of nonzeros                  = 1238244

 **** Sparse Matrix Assembled

 **** Invoking Parallel BCSLIB-EXT Sparse Solver...
 
 **** Load Cases 1

 **** Model checked through matrix assembly                                     
      Skip the rest of analysis. 
 
 
