

 Autodesk (R) Simulation Static Stress with Linear Material Models
 Version 2014.00.00.0206-W64/X64 08-Nov-2012
 Copyright (c) 2012, Autodesk, Inc. All rights reserved. 

------------------------------------------------- 
                          DATE: MARCH 28, 2013                
                          TIME: 11:18 AM
                   INPUT MODEL: D:\Autodesk Simulation Manuscript-13032013\c08_Autodesk-Simulation\tut01\c08_tut01.ds_data\1\ds

                    PROGRAM VERSION: 201400000206
            alg-win-x64.dll VERSION: 201400000206
       agsdb_ar-win-x64.dll VERSION: 201400000206
      algconfig-win-x64.dll VERSION: 201400000206
 solvercallback-win-x64.dll VERSION: 201400000206
               amgsolve.exe VERSION:    360000000
 
------------------------------------------------- 

 **** Model Unit System Settings:
      --------------------------------------------
       Unit System              : Custom
       Force                    : N
       Length                   : mm
       Time                     : s
       Temperature (Absolute)   : deg C (K)
       Thermal Energy           : J
       Voltage                  : V
       Current                  : A
       Electrical Resistance    : ohm
       Mass                     : N*s^2/mm
      --------------------------------------------

                                                  
1**** CONTROL INFORMATION                         
                                                  
      number of node points          (NUMNP)   =         17652
      number of element types        (NELTYP)  =             1
      number of load cases           (LL)      =             1
      number of frequencies          (NF)      =             0
      analysis type code             (NDYN)    =             0
      equations per block            (KEQB)    =             0
      bandwidth minimization flag    (MINBND)  =            -1
      gravitational constant         (GRAV)    =    9.8146E+03
      number of equations            (NEQ)     =         52676

 **** PRINT OF NODAL DATA SUPPRESSED              
 **** PRINT OF EQUATION NUMBERS SUPPRESSED        
 **** Read      72 MPC's from CST file
 **** Penalty based MPC method is used
 **** Hard disk file size information for processor:

      Available hard disk space on current drive = 401570.938 megabytes
      Gravity direction vector =  0.0000E+00  0.0000E+00 -1.0000E+00
                                                  
1**** ELEMENT LOAD MULTIPLIERS                    
                                                  
      load case      case A     case B     case C     case D     case E        
      ---------    ---------- ---------- ---------- ---------- ----------      
                                                  
          1         1.000E+00  0.000E+00  1.000E+00  0.000E+00  0.000E+00
  
      Centrifugal force / angular acceleration    
  
      load case     rot.rate   ang.acc.           
      ---------    ---------- ----------          
  
          1         0.000E+00  0.000E+00
  

 **** Symbolic Assembly Using the Row-Hits Matrix Profile ...
 **** Number of equations                 = 52676
      Estimated maximum bandwidth         = 2833
      Estimated triangle matrix nonzeroes = 12994427
      Symbolically assembled nonzeros     = 1238248
 **** Real Sparse Matrix Assembly ...
                                                  
1**** STIFFNESS MATRIX PARAMETERS                 
                                                  
      minimum non-zero diagonal element =           8.6634E+03
      maximum diagonal element          =           1.5840E+13
      maximum/minimum                   =           1.8284E+09
      average diagonal element          =           2.2081E+10
                                                  
      Minimum found at equation #52323: node = 17535 DOF=Tx
      Maximum found at equation #6002: node = 2022 DOF=Tz

      in the upper triangle:
      number of entries in the profile    = 12994643
      number of nonzeros                  = 1238244

 **** Sparse Matrix Assembled

 **** Invoking Parallel BCSLIB-EXT Sparse Solver...
 
 **** Load Cases 1

 **** Model checked through matrix assembly                                     
      Skip the rest of analysis.
