

 Autodesk (R) Simulation Static Stress with Linear Material Models
 Version 2015.00.00.0517-W64/X64 26-Feb-2014
 Copyright (c) 2014, Autodesk, Inc. All rights reserved. 

 
                          DATE: JULY 22, 2014                 
                          TIME: 10:28 AM
                   INPUT MODEL: D:\Autodesk Simulation Manuscript\Autodesk Simulation Manuscript 2015\Autodesk Simulation _Tut and Exe_Final - Used\Input File\c09_simulation_2014_input\Exe01\c08_exe01.ds_data\1\ds

                    PROGRAM VERSION: 201500000517
            alg-win-x64.dll VERSION: 201500000516
       agsdb_ar-win-x64.dll VERSION: 201500000516
      algconfig-win-x64.dll VERSION: 201500000516
 solvercallback-win-x64.dll VERSION: 201500000516
               amgsolve.exe VERSION:    360000000
 
 **** Linear stress analysis
 **** Nodes    | Parts | Loads | Freqs | Mode
          10803|      4|      1|      0|    0

 **** Model Unit System Settings:
      --------------------------------------------
       Unit System              : English (in)
       Force                    : lbf
       Length                   : in
       Time                     : s
       Temperature (Absolute)   : deg F (R)
       Thermal Energy           : in*lbf
       Voltage                  : V
       Current                  : A
       Electrical Resistance    : ohm
       Mass                     : lbf*s^2/in
      --------------------------------------------

  
      Options executed are: 
  
      NOMIN
      STRAIN
      SPARSE
      SUPCNF
      SUPELM
      SUPNOD
      REAC
  
  
      processing ... 
  
 **** OPENING TEMPORARY FILES
      NDYN = 0 
 **** BEGIN NODAL DATA INPUT
      10803 NODES
      32841 DOFS               
 **** END   NODAL DATA INPUT
 
 **** Begin brick element (TYPE-8) data input
 **** Part      1 containing      8380 elements
             0 ( 0.%) elements
                                                 
 **** End input of element part      1

 **** Begin brick element (TYPE-8) data input
 **** Part      2 containing       639 elements
                                                 
 **** End input of element part      2

 **** Begin brick element (TYPE-8) data input
 **** Part      3 containing     10548 elements
             0 ( 0.%) elements
                                                 
 **** End input of element part      3

 **** Begin beam element (TYPE-2) data input
 **** Part      4 containing       376 elements
                                                 
 **** End input of element part      4

 **** Hard disk file size information for processor:

      Available hard disk space on current drive = 121833.719 megabytes


 
 **** BEGIN LOAD INPUT
      Gravity direction vector =  0.0000E+00  0.0000E+00 -1.0000E+00
      One load case.
 **** END   LOAD INPUT

 **** Symbolic Assembly Using the Row-Hits Matrix Profile ...
 **** Number of equations                 = 32841
      Estimated maximum bandwidth         = 1708
      Estimated triangle matrix nonzeroes = 5113134
      Symbolically assembled nonzeros     = 848745
 **** Real Sparse Matrix Assembly ...
      in the upper triangle:
      number of entries in the profile    = 5113134
      number of nonzeros                  = 837570

 **** Sparse Matrix Assembled

 **** Invoking Parallel BCSLIB-EXT Sparse Solver...
 
 **** Load Cases 1
 **** End Sparse Solver Solution
 
 **** BEGIN DISPLACEMENT OUTPUT
 **** PRINT OF DISPLACEMENT OUTPUT SUPPRESSED
 **** END   DISPLACEMENT OUTPUT
 
 **** BEGINNING REACTION COMPUTATIONS
 **** LOADCASES REMAINING      1 
 **** PARTS REMAINING       4 
 **** ELEMENT/GLOBAL CONTRIBUTIONS Part = 1 
      THE 1st PART CONTAINING 8380 ELEMENTS
          7000 (83.%) elements
          6000 (71.%) elements
          5000 (59.%) elements
          4000 (47.%) elements
          3000 (36.%) elements
          2000 (24.%) elements
          1000 (12.%) elements
             0 ( 0.%) elements
                                                 
 **** PARTS REMAINING       3 
 **** ELEMENT/GLOBAL CONTRIBUTIONS Part = 2 
      THE 2nd PART CONTAINING 639 ELEMENTS
                                                 
 **** PARTS REMAINING       2 
 **** ELEMENT/GLOBAL CONTRIBUTIONS Part = 3 
      THE 3rd PART CONTAINING 10548 ELEMENTS
          8000 (75.%) elements
          6000 (57.%) elements
          4000 (38.%) elements
          2000 (19.%) elements
             0 ( 0.%) elements
                                                 
 **** PARTS REMAINING       1 
 **** ELEMENT/GLOBAL CONTRIBUTIONS Part = 4 
      THE 4th PART CONTAINING 376 ELEMENTS
                                                 
 **** ENDING REACTION COMPUTATIONS

      Processing completed ... 

 
      ds.t7    =     256.570 kilobytes
      ds.t8    =     506.496 kilobytes
      ds.t9    =       0.000 kilobytes
      ds.t10   =       0.000 kilobytes
      ds.t11   =       0.000 kilobytes
      ds.t12   =     256.570 kilobytes
      ds.t13   =     256.578 kilobytes
      ds.t14   =       0.000 kilobytes
      ds.t15   =       0.000 kilobytes
      ds.t17   =       0.000 kilobytes
      ds.t50   =   29717.805 kilobytes
      ds.t51   =    2475.250 kilobytes
      ds.t52   =   46245.086 kilobytes
      ds.t54   =     128.309 kilobytes
      ds.t55   =    3271.758 kilobytes
      ds.t56   =    6543.516 kilobytes
      ds.t56   =    6543.516 kilobytes
      ds.t58   =       0.000 kilobytes
      ds.t59   =       0.000 kilobytes
 
      total temporary disk storage (megabytes) = 93.947 
 
      ds.l     =       7.672 kilobytes
      ds.do    =     506.438 kilobytes
 
 **** BEGIN DELETING TEMPORARY FILES
 **** TEMPORARY FILES DELETED
 **** END OF SUCCESSFUL EXECUTION
 
 

 **** Total actual hard disk space used    =     94.449 megabytes

      Sub-total elapsed time               =      0.315 minutes



 Autodesk (R) Simulation Stress Calculation Utility
 Version 2015.00.00.0517-W64/X64 26-Feb-2014
 Copyright (c) 2014, Autodesk, Inc. All rights reserved. 


      DATE: JULY 22, 2014                 
      TIME: 10:28 AM
      INPUT......D:\Autodesk Simulation Manuscript\Autodesk Simulation Manuscript 2015\Autodesk Simulation _Tut and Exe_Final - Used\Input File\c09_simulation_2014_input\Exe01\c08_exe01.ds_data\1\ds 

 **** Model Unit System Settings:
      --------------------------------------------
       Unit System              : English (in)
       Force                    : lbf
       Length                   : in
       Time                     : s
       Temperature (Absolute)   : deg F (R)
       Thermal Energy           : in*lbf
       Voltage                  : V
       Current                  : A
       Electrical Resistance    : ohm
       Mass                     : lbf*s^2/in
      --------------------------------------------


 **** START PROCESSING ELEMENTS 

 **** BEGIN PART   1 TYPE( 8) ELEMENTS
      8380 ELEMENTS
          5308 (63.%) elements
          3260 (39.%) elements
          1212 (14.%) elements
                                                 
 **** BEGIN PART   2 TYPE( 8) ELEMENTS
      639 ELEMENTS
                                                 
 **** BEGIN PART   3 TYPE( 8) ELEMENTS
      10548 ELEMENTS
          6452 (61.%) elements
          5428 (51.%) elements
          2048 (19.%) elements
                                                 
 **** BEGIN PART   4 TYPE( 2) ELEMENTS
      376 ELEMENTS
                                                 

 **** FINISHED PROCESSING ELEMENTS 

 **** Hard disk file size information for postprocessor:
      ds.nso   =    5532.746 kilobytes
      ds.sto   =    5532.746 kilobytes

      Total MKNSO disk space used        =    10.80614 megabytes
 **** MKNSO elapsed time                 =       0.068 minutes

 **** The TOTAL elapsed time             =       0.383 minutes

 
