fem2esh - Make esh file from fem file for a specified design scenario
Version 2014.00.00.0513-W64/X64 22-Feb-2013
Copyright (c) 2013, Autodesk, Inc. All rights reserved.

  Version of fem2esh.exe          : 2014.00000513
  Version of dcx1-win-x64.dll     : 2014.00000513
  Version of femapi-win-x64.dll   : 2014.00000513
  Version of agsdb_ar-win-x64.dll : 2014.00000513
  Version of tsx2tsy.exe          : 2014.00000513

  Input Model     : D:\Autodesk Simulation Manuscript\c08_Autodesk-Simulation\tut01\c08_tut01.ds_data\1\ds
  Input File      : D:\Autodesk Simulation Manuscript\c08_Autodesk-Simulation\tut01\c08_tut01.fem
  Output File     : D:\Autodesk Simulation Manuscript\c08_Autodesk-Simulation\tut01\c08_tut01.ds_data\1\ds.mod\group.esh
  Log File        : D:\Autodesk Simulation Manuscript\c08_Autodesk-Simulation\tut01\c08_tut01.ds_data\1\ds.mod\group.ldx
  Design scenario : 1
  Analysis type   : Linear Stress
  Start time      : 2013/05/15-12:49:29  

  --- Get one active element part from fem file
  --- 3 enabled L&C groups are defined
  --- Get 41163 points defined in range [1, 41163] from fem file
  Calling the Surface Topology Generator (tsx2tsy)...
  tsx2tsy: Update part surface contact/bonding data (duration=1 sec.)
  --- No mid-side node required
  Set up nodal properties such as admissible BC etc. by adjacent elements...
  --- No non-trivial coincident nodal pairs of 0 in FEM
  Consolidate points between parts using contact definitions...
  --- No contact used from 0 contact definitions
  Compress FEM points to ESH nodes...
  --- Found 17652 independent nodes
  --- 17652 mesh nodes formed from 41163 FEM points
  Output the mapping arrays of FEM points to FEA nodes...
  Add user defined nodal B.C.'s...
  --- 140 Pin Constrained points
  --- No contact found
  Get beam loads and constraints data...
  Writing to ESH file in phase I (nodes & elements)...
  --- Part1: type=8, flags=7, meshType=10, elements=50826, maximumID=50826
  Working on MPCs...
  Working on 1 defined surface frictionless constraint objects...
  --- Output 72 MPC for surface frictionless constraint#1
  --- Made total 72 enabled MPCs.
  Writing to ESH file in phase II (FEA objects)...

  Writing 2 coordinate systems (nodal.lcs).


  == Model Stats ==

  FEA Nodes & Elements:
  --- 17652 mesh nodes
  --- One part and 50826 elements
  FEA Object: None
  FEM2ESH Duration: 2 seconds (CPU time)

2013/05/15-12:49:31