

 Autodesk (R) Simulation Static Stress with Linear Material Models
 Version 2014.00.00.0513-W64/X64 22-Feb-2013
 Copyright (c) 2013, Autodesk, Inc. All rights reserved. 

 
                          DATE: MAY 15, 2013                  
                          TIME: 12:50 PM
                   INPUT MODEL: D:\Autodesk Simulation Manuscript\c08_Autodesk-Simulation\tut01\c08_tut01.ds_data\1\ds

                    PROGRAM VERSION: 201400000513
            alg-win-x64.dll VERSION: 201400000513
       agsdb_ar-win-x64.dll VERSION: 201400000513
      algconfig-win-x64.dll VERSION: 201400000513
 solvercallback-win-x64.dll VERSION: 201400000513
               amgsolve.exe VERSION:    360000000
 
 **** Linear stress analysis
 **** Nodes    | Parts | Loads | Freqs | Mode
          17652|      1|      1|      0|    0

 **** Model Unit System Settings:
      --------------------------------------------
       Unit System              : Custom
       Force                    : N
       Length                   : mm
       Time                     : s
       Temperature (Absolute)   : deg C (K)
       Thermal Energy           : J
       Voltage                  : V
       Current                  : A
       Electrical Resistance    : ohm
       Mass                     : N*s^2/mm
      --------------------------------------------

  
      Options executed are: 
  
      NOMIN
      STRAIN
      SPARSE
      SUPCNF
      SUPELM
      SUPNOD
      REAC
  
  
      processing ... 
  
 **** OPENING TEMPORARY FILES
      NDYN = 0 
 **** BEGIN NODAL DATA INPUT
      17652 NODES
      52676 DOFS               
 **** END   NODAL DATA INPUT
 
 **** Read      72 MPC's from CST file
 **** Penalty based MPC method is used
 **** Begin brick element (TYPE-8) data input
 **** Part      1 containing     50827 elements
         48000 (94.%) elements
         46000 (90.%) elements
         44000 (86.%) elements
         42000 (82.%) elements
         40000 (78.%) elements
         38000 (74.%) elements
         36000 (70.%) elements
         34000 (67.%) elements
         32000 (63.%) elements
         30000 (59.%) elements
         28000 (55.%) elements
         26000 (51.%) elements
         24000 (47.%) elements
         22000 (43.%) elements
         20000 (39.%) elements
         18000 (35.%) elements
         16000 (31.%) elements
         14000 (27.%) elements
         12000 (23.%) elements
         10000 (20.%) elements
          8000 (16.%) elements
          6000 (12.%) elements
          4000 ( 8.%) elements
          2000 ( 4.%) elements
             0 ( 0.%) elements
                                                 
 **** End input of element part      1

 **** Hard disk file size information for processor:

      Available hard disk space on current drive =  67045.305 megabytes


 
 **** BEGIN LOAD INPUT
      Gravity direction vector =  0.0000E+00  0.0000E+00 -1.0000E+00
      One load case in 3 blocks.
 **** END   LOAD INPUT

 **** Symbolic Assembly Using the Row-Hits Matrix Profile ...
 **** Number of equations                 = 52676
      Estimated maximum bandwidth         = 2833
      Estimated triangle matrix nonzeroes = 12994427
      Symbolically assembled nonzeros     = 1238248
 **** Real Sparse Matrix Assembly ...
      in the upper triangle:
      number of entries in the profile    = 12994643
      number of nonzeros                  = 1238244

 **** Sparse Matrix Assembled

 **** Invoking Parallel BCSLIB-EXT Sparse Solver...
 
 **** Load Cases 1
 **** End Sparse Solver Solution
 
 **** BEGIN DISPLACEMENT OUTPUT
 **** PRINT OF DISPLACEMENT OUTPUT SUPPRESSED
 **** END   DISPLACEMENT OUTPUT
 
 **** BEGINNING REACTION COMPUTATIONS
 **** LOADCASES REMAINING      1 
 **** PARTS REMAINING       1 
 **** ELEMENT/GLOBAL CONTRIBUTIONS Part = 1 
      THE 1st PART CONTAINING 50827 ELEMENTS
         48000 (94.%) elements
         46000 (90.%) elements
         44000 (86.%) elements
         42000 (82.%) elements
         40000 (78.%) elements
         38000 (74.%) elements
         36000 (70.%) elements
         34000 (67.%) elements
         32000 (63.%) elements
         30000 (59.%) elements
         28000 (55.%) elements
         26000 (51.%) elements
         24000 (47.%) elements
         22000 (43.%) elements
         20000 (39.%) elements
         18000 (35.%) elements
         16000 (31.%) elements
         14000 (27.%) elements
         12000 (23.%) elements
         10000 (20.%) elements
          8000 (16.%) elements
          6000 (12.%) elements
          4000 ( 8.%) elements
          2000 ( 4.%) elements
             0 ( 0.%) elements
                                                 
 **** ENDING REACTION COMPUTATIONS

      Processing completed ... 

 
      ds.t7    =     411.539 kilobytes
      ds.t8    =     827.543 kilobytes
      ds.t9    =       0.000 kilobytes
      ds.t10   =       0.000 kilobytes
      ds.t11   =       0.000 kilobytes
      ds.t12   =     411.531 kilobytes
      ds.t13   =     411.562 kilobytes
      ds.t14   =       0.000 kilobytes
      ds.t15   =       0.000 kilobytes
      ds.t17   =       0.000 kilobytes
      ds.t50   =   76637.586 kilobytes
      ds.t51   =    6353.375 kilobytes
      ds.t52   =  119522.867 kilobytes
      ds.t54   =     205.789 kilobytes
      ds.t55   =    4836.891 kilobytes
      ds.t56   =    9673.781 kilobytes
      ds.t56   =    9673.781 kilobytes
      ds.t58   =       0.000 kilobytes
      ds.t59   =       0.000 kilobytes
 
      total temporary disk storage (megabytes) = 223.600 
 
      ds.l     =       7.086 kilobytes
      ds.do    =     827.484 kilobytes
 
 **** BEGIN DELETING TEMPORARY FILES
 **** TEMPORARY FILES DELETED
 **** END OF SUCCESSFUL EXECUTION
 
 

 **** Total actual hard disk space used    =    224.415 megabytes

      Sub-total elapsed time               =      1.041 minutes



 Autodesk (R) Simulation Stress Calculation Utility
 Version 2014.00.00.0513-W64/X64 22-Feb-2013
 Copyright (c) 2013, Autodesk, Inc. All rights reserved. 


      DATE: MAY 15, 2013                  
      TIME: 12:51 PM
      INPUT......D:\Autodesk Simulation Manuscript\c08_Autodesk-Simulation\tut01\c08_tut01.ds_data\1\ds 

 **** Model Unit System Settings:
      --------------------------------------------
       Unit System              : Custom
       Force                    : N
       Length                   : mm
       Time                     : s
       Temperature (Absolute)   : deg C (K)
       Thermal Energy           : J
       Voltage                  : V
       Current                  : A
       Electrical Resistance    : ohm
       Mass                     : N*s^2/mm
      --------------------------------------------


 **** START PROCESSING ELEMENTS 

 **** BEGIN PART   1 TYPE( 8) ELEMENTS
      50827 ELEMENTS
         48779 (95.%) elements
         47755 (93.%) elements
         46731 (91.%) elements
         45707 (89.%) elements
         44683 (87.%) elements
         43659 (85.%) elements
         42635 (83.%) elements
         41611 (81.%) elements
         40587 (79.%) elements
         39563 (77.%) elements
         38539 (75.%) elements
         37515 (73.%) elements
         36491 (71.%) elements
         35467 (69.%) elements
         34443 (67.%) elements
         33419 (65.%) elements
         32395 (63.%) elements
         31371 (61.%) elements
         30347 (59.%) elements
         29323 (57.%) elements
         28299 (55.%) elements
         27275 (53.%) elements
         26251 (51.%) elements
         25227 (49.%) elements
         24203 (47.%) elements
         23179 (45.%) elements
         22155 (43.%) elements
         21131 (41.%) elements
         20107 (39.%) elements
         19083 (37.%) elements
         18059 (35.%) elements
         17035 (33.%) elements
         16011 (31.%) elements
         14987 (29.%) elements
         13963 (27.%) elements
         12939 (25.%) elements
         11915 (23.%) elements
         10891 (21.%) elements
          9867 (19.%) elements
          8843 (17.%) elements
          7819 (15.%) elements
          6795 (13.%) elements
          5771 (11.%) elements
          4747 ( 9.%) elements
          3723 ( 7.%) elements
          2699 ( 5.%) elements
          1675 ( 3.%) elements
           651 ( 1.%) elements
                                                 

 **** FINISHED PROCESSING ELEMENTS 

 **** Hard disk file size information for postprocessor:
      ds.nso   =   14295.164 kilobytes
      ds.sto   =   14295.164 kilobytes

      Total MKNSO disk space used        =    27.92024 megabytes
 **** MKNSO elapsed time                 =       1.001 minutes

 **** The TOTAL elapsed time             =       2.042 minutes

 
