



_________________________________________________



    SOLID MESH GENERATION BEFORE ANALYSIS   

_________________________________________________



PROGRAM WILL USE THE FOLLOWING FILES:

    Input:  D:\Autodesk Simulation Manuscript-13032013\c08_Autodesk-Simulation\tut02\c08_tut02.FEM

    Output: D:\Autodesk Simulation Manuscript-13032013\c08_Autodesk-Simulation\tut02\c08_tut02.FEM


COMMAND LINE:
    C:\Program Files\Autodesk\Simulation 2014\SOLIDX.exe -b=0 -o=1 -zw=2 D:\Autodesk Simulation Manuscript-13032013\c08_Autodesk-Simulation\tut02\c08_tut02 -ds=1 -d=0 -u=13 -c=2 -t=1 -progress_pipe=4 -cancel_pipe=5 -za=-1 -zg=1:2 -m=2 -Td=1 -Tl=2 -Tg=1.2 -Tq=100 -L 


TYPE OF OPERATION:  

    Meshing only surface defined by part 2

    Generating bricks, wedges, pyramids and tetrahedra elements

    Automatically minimizing aspect ratio of solid elements





FINAL STATISTICS:

    Elements built (4,5,6,8 noded): 9463  ( 3358, 1478, 597, 4030 )

    Volume (4,5,6,8 noded %): 31252.761612 (   5.70,   5.40,   5.18,  83.73 )

    Number of nodes: 7813

    Length ratios (avg)     4.9,     3.5,     1.8,     1.3
    Length ratios (max)   614.5,    25.4,     7.0,     4.3
    Aspect ratio: unconstrained (   5.3,   3.6,   1.6,   1.2 )
    Average aspect ratios:      (   1.3,   1.3,   1.1,   1.0 )
    Number of restarts:   0
    Elapsed time: 0 minutes 7 seconds







_________________________________________________





    SOLID MESH GENERATION BEFORE ANALYSIS   


_________________________________________________





PROGRAM WILL USE THE FOLLOWING FILES:


    Input:  D:\Autodesk Simulation Manuscript-13032013\c08_Autodesk-Simulation\tut02\c08_tut02.FEM


    Output: D:\Autodesk Simulation Manuscript-13032013\c08_Autodesk-Simulation\tut02\c08_tut02.FEM




COMMAND LINE:

    C:\Program Files\Autodesk\Simulation 2014\SOLIDX.exe -b=0 -o=1 -zw=2 D:\Autodesk Simulation Manuscript-13032013\c08_Autodesk-Simulation\tut02\c08_tut02 -ds=1 -d=0 -u=13 -c=2 -t=1 -progress_pipe=8 -cancel_pipe=9 -za=-1 -zg=1:2 -m=1 -Td=1 -Tl=2 -Tg=1.2 -Tq=100 -L 




TYPE OF OPERATION:  


    Meshing only surface defined by part 1


    Generating bricks, wedges, pyramids and tetrahedra elements


    Automatically minimizing aspect ratio of solid elements








FINAL STATISTICS:


    Elements built (4,5,6,8 noded): 10409  ( 4830, 2203, 582, 2794 )


    Volume (4,5,6,8 noded %): 27134.723727 (   6.42,   7.24,   6.30,  80.05 )


    Number of nodes: 6893


    Length ratios (avg)     6.1,     4.0,     2.0,     1.5

    Length ratios (max)   216.0,    78.0,     6.3,     6.7

    Aspect ratio: unconstrained (   3.9,   3.6,   1.4,   1.3 )

    Average aspect ratios:      (   1.3,   1.3,   1.1,   1.0 )

    Number of restarts:   0

    Elapsed time: 0 minutes 13 seconds



